***Quick and easy for you - please fill out areas highlighted in green to complete the specification***

**PART 1 GENERAL**

# RELATED DOCUMENTS

## Drawings and general conditions of the contract, including general and supplementary conditions and division 1 specification sections, apply to the work of this section.

# SUMMARY

## Section includes:

### Sound absorptive baffles

## Related sections

### Section 01350 – Special Environmental Requirements

### Section 095300 – Acoustical Ceiling Suspension Systems (by others)

### Section 095100 – Acoustical Ceilings

### Section 092116 – Gypsum Board Assemblies (by others)

### Section 09800 – Acoustical Treatment

# SUBMITTALS

## Comply with Section 013300 – Submittal Procedures

## **Product Data:** Manufacturer’s technical data and installation instructions for each type of ceiling baffle required.

## **Certifications:** Certified test reports showing compliance with performance requirements specified.

## **Samples:** Submit a minimum of one (1) sample of each panel type and finish type required.

## **Shop Drawings:** Submit shop drawings when applicable. When necessary include details, for all ceilings, coordinate ceiling baffle layout, installation and suspension system components, and show overall layout with dimensions and details of penetrations and intersections with other materials or building components.

## **LEED Requirements:** Where specified, submit required documentation indicating compliance.

## Submit operation and maintenance data for installed products. Include precautions relating to harmful cleaning materials and methods that would affect the service life of the baffles.

# QUALITY ASSURANCE

## A. **Single Source Responsibility:** Provide acoustic bafflesfrom a single manufacturer with at least 5 years of prior experience fabricating projects of similar size and complexity.

## **Installer:** Installation shall be done by qualified contractors with at least two (2) years experience in the installation of acoustical ceilings. Installers should receive training on handling and field finishing the specified product prior to receiving materials on site.

## **Fire Performance Characteristics:** Class A as tested by an independent accredited testing facility. Tests: ASTM E84. Flame spread: 25 or less. Smoke developed: 450 or less as specified by state or local codes.

## **Applicable LEED Credits:**

### MRc4 Recycled Content

### EQ 9 Enhanced Acoustical Performance

## **Coordination of Work:** Installing contractor shall organize and conduct a pre-installation survey of temperature, humidity and construction elements attaching, penetrating or concealed behind the acoustic baffles.

# 1.5 REFERENCES

## A. **Test Methods:**

### **ASTM C423** Sound absorption and sound absorption coefficients by the reverberation room method performed by an independent testing agency

### **ASTM E84** Standard test method for surface burning characteristics of building materials

# 1.6 DELIVERY, STORAGE AND HANDLING

## A. Deliver baffles to the project in original, unopened packages. Inspect containers for visible damage and report any questionable condition to the shipper and manufacturer immediately.

## Store products in a fully enclosed, clean, dry space out of direct sunlight and protected from damage with temperature controlled between 50 and 86 degrees F.

## Handle products carefully to avoid damaging baffle surfaces or chipping edges. Report any damage immediately. Installation of damaged baffles is not covered by the manufacturer’s warranty.

# PROJECT CONDITIONS

## Do not install acoustic ceiling bafflesuntil space is enclosed and weather-proofed, wet work is completely dry and ambient temperature and humidity conditions are maintained at the levels indicated for the project when occupied for its intended use.

## Permit baffles to reach room temperature, 50 to 86 degrees F, and stabilized moisture content of 25% to 55% RH for at least 72 hours before installation per AWI standards. Building should be enclosed and HVAC systems functioning in continuous operation with relative humidity maintained between 25 and 55 percent.

# WARRANTY

## Provide manufacturer’s standard **three (3) year written product warranty** per Section 01770 – Closeout Procedures

## Manufacturer’s warranty is limited to decorative or acoustical baffle materials only. Other components used in the ceiling system are excluded. Refer to the appropriate provisions in the related specification section.

# MAINTENANCE

## **Maintenance Instructions:** Provide manufacturer’s standard maintenance and cleaning instructions for finishes provided.

# PART 2 – PRODUCTS

# MANUFACTURER

## Provide baffles utilizing SONUS acoustic panels manufactured by Sonus North America, LLC 7601 Miller Drive, Frederick, CO 80504, Ph. (303) 774-9992, email [sales@sonusna.com.](mailto:sales@sonusna.com.)

# MATERIALS

**SONUS Baffles for Interior Installation: Select**Kowen (2.25”) or Kowen (4.25”) thick acoustical baffles as follows: Factory-applied latex paint (or digital print option) on a rigid, resilient fiberglass board manufactured using flame-attenuated glass fibers with CX17 mat facing that has been precisely CNC machined to enable folding and wrapping in order to provide a linear and upscale visual. The core of the baffles shall be comprised of Class A 6-7 pcf fiberglass.

## **Baffle Weight:** 2.25” =1.2 lbs/ft2, 4.25 = 2.1 lbs/ft2

## **Baffle Sizes:** **Select** Baffles are available in the following sizes:

## Baffle Height: *(nominal 9”, 12”, 16”)*

## Baffle Length: *(46”or 94”)*

## Baffle Width: *(2.25”or 4.25”)*

## **Flame Resistance:** SONUS Baffles have a Class 1(A) rating for surface burning characteristics in building materials.

## **Acoustic Performance:** To generate the standing sound waves required for resistive absorption, each baffle must contain a rigid, acoustically reflective, center barrier wall that extends the baffle’s full length and height. With the center barrier wall installed, each side of the baffle must achieve minimum NRC test values as stated: 2.5” thick - 1.35 NRC.

## **Finish: Select**

### Painted – see standard colors on website or provide pantone code for custom application

### Digitally Printed (high resolution image provided by specifier or client)

# PART 3 – EXECUTION/ft2

# EXAMINATION

## Inspect installation area and conditions under which work is to be performed for compliance with all manufacturer’s environmental requirements. All wet work in the installation area must be complete, cured and dry prior to installation. Do not proceed until all unsatisfactory conditions have been corrected.

# INSTALLATION

## Installation must be done by qualified contractor with 2 years experience in the installation of acoustic ceilings. The firm must demonstrate successful experience installing materials of similar type and quality of those required for this project.

## Comply with manufacturer’s instruction and recommendations for hanging baffles.

* 1. For suspended grid, install adjustable coupler, suspension cable, and choice of grid mounting hardware.

* 1. For direct mount, install using direct cable suspension with adjustable coupler, suspension cable, and panel anchors.

## Confirm all field dimensions are coordinated with shop drawings.

# ADJUSTING AND CLEANING

## Clean soiled surfaces of baffles per manufacturer’s instructions.

## Remove and replace damaged or discolored materials not in compliance with manufacturer’s tolerances.

# Contact information:

Sonus North America

7601 Miller Drive

Frederick, CO 80504

303-774-9992

[sales@sonusna.com](mailto:sales@sonusna.com)

# END OF SECTION